[bookmark: X45dd9449270c3265b5db9a9f6a36324e803afff][bookmark: _Toc48238035]Supplementary Figure S6: Receiver operating characteristics curves of the AUDIT-C, full AUDIT, and EWAC on consumption thresholds from the GF reference standard
Note: The raw data for every ROC curve are available from the repository https://github.com/peterdutey/ewac-validation/tree/master/04_suppmat/ROC 
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