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Supplemental Figure 1: Schematic of the passive inhalation chambers. A suction air pump draws air through an intake port and pulls vapor from a tank containing the vape oil. The air and vapor then is pulled evenly through 4 inhalation chambers and then pushed out to a fume hood. The heating element is controlled by a computer and aerosolizes the contents of the oil leading to vapor entering the chambers.  
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